Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package opencard.opt.iso.fs

Interface Summary
CardFileInfo | Provides information about the structure of a file.
FileAccessCardService | Interface to a card service for ISO 7816-4 file access functionality.
FileSystemCardService | Interface defining creational methods for file system based smartcards.

Class Summary
CardFile | Represents a file or directory on the smartcard.
CardFileAppID | `CardFileAppID` contains a single `CardFilePath` component, an application ID.
CardFileFileID | `CardFileFileID` contains a single `CardFilePath` component, a two byte file ID.
CardFileInputStream | `CardFileInputStream` together with the accompanying `CardFileOutputStream` provides access to a `CardFile` via the familiar Java input/output stream mechanism. This class only works on transparent files.
CardFileOutputStream | `CardFileInputStream` together with the accompanying `CardFileOutputStream` provides access to a `CardFile` via the familiar Java input/output stream mechanism.
CardFilePartialAppID | `CardFilePartialAppID` contains a single `CardFilePath` component, a partial application ID.
CardFilePath | `CardFilePath` encapsulates the various ways of addressing files on a smart card: File ID paths: A sequence of two byte file IDs as defined in ISO 7816-4 Short File ID: One byte short file ID (0..31) for selecting EFs.
CardFilePathComponent | `CardFilePathComponent` contains a single `CardFilePath` component.
CardFileReader | `CardFileReader` is a subclass of `InputStreamReader` that can be used to read text data from a `CardFile`.
CardFileShortFileID | `CardFileShortFileID` contains a single `CardFilePath` component, a short file ID.
CardFileSymbolicName | `CardFileSymbolicName` contains a single `CardFilePath` component, a symbolic name.
CardFileWriter | `CardFileWriter` is a subclass of `OutputStreamWriter` that can be used to read text data from a `CardFile`.
CardRandomAccess | Superclass for both `CardRandomAccess` classes.
CardRandomByteAccess | `CardRandomByteAccess` provides a byte-oriented way of accessing a card file (for transparent smart card files).
CardRandomRecordAccess | `CardRandomRecordAccess` provides record-oriented, random access to structured smart card files.
CardRecord | The `CardRecord` class is used by the `CardRandomRecordAccess` and `CardRandomByteAccess` classes.

Exception Summary
CardIOException | `CardIOException` is the base class for all `CardIO` related exceptions.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES