Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package opencard.opt.applet

Interface Summary
AppletSelector | The `AppletSelector` interface defines the minimum features that are necessary for working with card-resident applets.

Class Summary
AppletID | `AppletID` encapsulates the applet identifier as defined by ISO 7816-5.
AppletInfo | The `AppletInfo` encapsulates the descriptive information about an applet stored on a smart card (e.g. security Domain or AppletID).
AppletProxy | `AppletProxy` is the base class for all applet proxies.
AppletState | Applet states are to be used for representing the state of an applet to applet proxies associated with that applet.
BasicAppletCardService | This service offers methods to applications or proxies derived from it, which send a given command APDU to the card applet identified by the given application identifier and which return the result APDU.
CardState | Encapsulates the state of a multi-applicative card.
ID | ID - A wrapper class for unsigned byte arrays.
ISOAppletSelector | The `ISOAppletSelector` is a class providing the `selectApplet` functionality as specified in the `AppletSelector` interface.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES