Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package opencard.opt.terminal

Interface Summary
Lockable | `Lockable` is a generic interface for locking a terminal or individual slots.
PowerManagementInterface | A `CardTerminal` that implements the `PowerMangementInterface` can power down and power up the smart card in a slot.
TerminalCommand | `TerminalCommand` is a generic interface for sending commands to a `CardTerminal`.
UserInteraction | User interaction takes place through the `display()` method (to display information to the user), the `keyboardInput()` method (to retrieve information from the user) and the `promptUser()` method to combine display and input in a single call.

Class Summary
AbstractLockableTerminal | `AbstractLockableTerminal` is a base class for implementing lockable CardTerminals.
ISOCommandAPDU |

Exception Summary
TerminalLockedException | A `TerminalLockedException` signals that an operation was requested from a locked terminal by another thread than the lock owner.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES